(footprint "C_0402"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -1.16 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "803c088f-c347-4396-9819-66e0d1bfbf37")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 1.16 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "176d1865-3c67-4dcb-8244-61d1b3f7d43f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "107cc154-f98f-4f44-92a6-626d8b8b4cc9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Unpolarized capacitor"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7fc0cd5-83e4-47f7-b6b0-232e4b2a6492")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Part" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2ac7d86e-b2e3-4cd4-96ef-f93f993b72b4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.05 -0.37)
		(end 0.05 -0.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b8efc763-72e4-4822-b6e0-05659e4c646c")
	)
	(fp_line
		(start -0.05 0.37)
		(end 0.05 0.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aeb3538d-941e-40cb-917d-e47093a0d89b")
	)
	(fp_line
		(start -0.91 -0.46)
		(end 0.91 -0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5dac8ef3-7a36-44ee-8025-cca5816b6d61")
	)
	(fp_line
		(start -0.91 0.46)
		(end -0.91 -0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97038f07-5c42-488c-b0d0-b7ed75d3a9c2")
	)
	(fp_line
		(start 0.91 -0.46)
		(end 0.91 0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f088d1f7-32bd-42f2-8828-f24ec35b3cdf")
	)
	(fp_line
		(start 0.91 0.46)
		(end -0.91 0.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6542880c-0feb-43ab-94e1-9a0838892257")
	)
	(fp_line
		(start -0.5 -0.25)
		(end 0.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "40015823-0556-488b-91cc-fe88076efed9")
	)
	(fp_line
		(start -0.5 0.25)
		(end -0.5 -0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "87dbea5e-ecd9-4088-ac91-4d4f5d21d92d")
	)
	(fp_line
		(start 0.5 -0.25)
		(end 0.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "337ee576-0302-4bd9-a162-4d143b8fd849")
	)
	(fp_line
		(start 0.5 0.25)
		(end -0.5 0.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2d0c4e3a-714f-47f7-b33c-15e63679198c")
	)
	(fp_text user "REF**"
		(at 0 -0.7 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0a42ee12-f886-49d8-bd84-843661dd9ba8")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.04)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "d940cb01-609e-4d20-9e17-177e7ac840db")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.04)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.48 0)
		(size 0.56 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "10b97ca8-1faa-4ac5-ab6f-b0c32f330191")
	)
	(pad "2" smd roundrect
		(at 0.48 0)
		(size 0.56 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "2d45dd4f-5465-4d11-9d1a-c4b787a56be3")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
