(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32F042C6T6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Value" "STM32F042C6T6"
			(at 0 3.302 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Footprint" "STM32F042C6T6:QFP50P700X700X160-48N"
			(at 0 5.842 0)
			(do_not_autoplace)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "STM32F042C6T6_1_0"
			(pin power_in line
				(at 2.54 2.54 270)
				(length 2.54)
				(name "VBAT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 2.54 270)
				(length 2.54)
				(name "VDD1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 -16.51 90)
				(length 2.54)
				(name "VSS1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 10.16 2.54 270)
				(length 2.54)
				(name "VDD2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 10.16 -16.51 90)
				(length 2.54)
				(name "VSS2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 2.54 270)
				(length 2.54)
				(name "VDDIO2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -16.51 90)
				(length 2.54)
				(name "VSS3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 2.54 270)
				(length 2.54)
				(name "VDDA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 20.32 -16.51 90)
				(length 2.54)
				(name "VSSA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "STM32F042C6T6_1_1"
			(rectangle
				(start 0 0)
				(end 22.86 -13.97)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type color)
					(color 255 255 194 1)
				)
			)
		)
		(symbol "STM32F042C6T6_2_0"
			(pin input line
				(at -2.54 -5.08 0)
				(length 2.54)
				(name "PF11-BOOT0"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "PC13/WKUP2/RTC_TAMP1/RTC_TS/RTC_OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "PC14-OSC32_IN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -15.24 0)
				(length 2.54)
				(name "PC15-OSC32_OUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -20.32 0)
				(length 2.54)
				(name "PF0-OSC_IN/CRS_SYNC/I2C1_SDA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -22.86 0)
				(length 2.54)
				(name "PF1-OSC_OUT/I2C1_SCL"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "STM32F042C6T6_2_1"
			(rectangle
				(start 0 0)
				(end 35.56 -25.4)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type color)
					(color 255 255 194 1)
				)
			)
			(pin input line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "~{NRST}"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "STM32F042C6T6_3_0"
			(pin bidirectional line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "PA0/USART2_CTS/TIM2_CH1_ETR/TSC_G1_IO1/RTC_TAMP2/WKUP1/ADC_IN0"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -5.08 0)
				(length 2.54)
				(name "PA1/USART2_RTS/TIM2_CH2/TSC_G1_IO2/EVENTOUT/ADC_IN1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -7.62 0)
				(length 2.54)
				(name "PA2/USART2_TX/TIM2_CH3/TSC_G1_IO3/ADC_IN2/WKUP4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "PA3/USART2_RX/TIM2_CH4/TSC_G1_IO4/ADC_IN3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "PA4/SPI1_NSS/I2S1_WS/TIM14_CH1/TSC_G2_IO1/USART2_CK/USB_NOE/ADC_IN4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -15.24 0)
				(length 2.54)
				(name "PA5/SPI1_SCK/I2S1_CK/CEC/TIM2_CH1_ETR/TSC_G2_IO2/ADC_IN5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -17.78 0)
				(length 2.54)
				(name "PA6/SPI1_MISO/I2S1_MCK/TIM3_CH1/TIM1_BKIN/TIM16_CH1/TSC_G2_IO3/EVENTOUT/ADC_IN6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -20.32 0)
				(length 2.54)
				(name "PA7/SPI1_MOSI/I2S1_SD/TIM3_CH2/TIM14_CH1/TIM1_CH1N/TIM17_CH1/TSC_G2_IO4/EVENTOUT/ADC_IN7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -22.86 0)
				(length 2.54)
				(name "PA8/USART1_CK/TIM1_CH1/EVENTOUT/MCO/CRS_SYNC"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -25.4 0)
				(length 2.54)
				(name "PA9/USART1_TX/TIM1_CH2/TSC_G4_IO1/I2C1_SCL"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -27.94 0)
				(length 2.54)
				(name "PA10/USART1_RX/TIM1_CH3/TIM17_BKIN/TSC_G4_IO2/I2C1_SDA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -30.48 0)
				(length 2.54)
				(name "PA11/CAN_RX/USART1_CTS/TIM1_CH4/COMP1_OUT/TSC_G4_IO3/EVENTOUT/I2C1_SCL/USB_DM"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -33.02 0)
				(length 2.54)
				(name "PA12/CAN_TX/USART1_RTS/TIM1_ETR/TSC_G4_IO4/EVENTOUT/I2C1_SDA/USB_DP"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -35.56 0)
				(length 2.54)
				(name "PA13/IR_OUT/SWDIO/USB_NOE"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -38.1 0)
				(length 2.54)
				(name "PA14/USART2_TX/SWCLK"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -40.64 0)
				(length 2.54)
				(name "PA15/SPI1_NSS/I2S1_WS/USART2_RX/TIM2_CH1_ETR/EVENTOUT/USB_NOE"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "STM32F042C6T6_3_1"
			(rectangle
				(start 0 0)
				(end 83.82 -43.18)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type color)
					(color 255 255 194 1)
				)
			)
		)
		(symbol "STM32F042C6T6_4_0"
			(pin bidirectional line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "PB0/TIM3_CH3/TIM1_CH2N/TSC_G3_IO2/EVENTOUT/ADC_IN8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -5.08 0)
				(length 2.54)
				(name "PB1/TIM3_CH4/TIM14_CH1/TIM1_CH3N/TSC_G3_IO3/ADC_IN9"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -7.62 0)
				(length 2.54)
				(name "PB2/TSC_G3_IO4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "PB3/SPI1_SCK/I2S1_CK/TIM2_CH2/TSC_G5_IO1/EVENTOUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "PB4/SPI1_MISO/I2S1_MCK/TIM17_BKIN/TIM3_CH1/TSC_G5_IO2/EVENTOUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -15.24 0)
				(length 2.54)
				(name "PB5/SPI1_MOSI/I2S1_SD/I2C1_SMBA/TIM16_BKIN/TIM3_CH2/WKUP6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -17.78 0)
				(length 2.54)
				(name "PB6/I2C1_SCL/USART1_TX/TIM16_CH1N/TSC_G5_I03"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -20.32 0)
				(length 2.54)
				(name "PB7/I2C1_SDA/USART1_RX/USART4_CTS/TIM17_CH1N/TSC_G5_IO4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -22.86 0)
				(length 2.54)
				(name "PB8/I2C1_SCL/CEC/TIM16_CH1/TSC_SYNC/CAN_RX"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -25.4 0)
				(length 2.54)
				(name "PB9/SPI2_NSS/I2C1_SDA/IR_OUT/TIM17_CH1/EVENTOUT/CAN_TX"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -27.94 0)
				(length 2.54)
				(name "PB10/SPI2_SCK/CEC/TSC_SYNC/TIM2_CH3/I2C1_SCL"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -30.48 0)
				(length 2.54)
				(name "PB11/TIM2_CH4/EVENTOUT/I2C1_SDA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -33.02 0)
				(length 2.54)
				(name "PB12/TIM1_BKIN/SPI2_NSS/EVENTOUT"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -35.56 0)
				(length 2.54)
				(name "PB13/SPI2_SCK/TIM1_CH1N/I2C1_SCL"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -38.1 0)
				(length 2.54)
				(name "PB14/SPI2_MISO/TIM1_CH2N/I2C1_SDA"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -40.64 0)
				(length 2.54)
				(name "PB15/SPI2_MOSI/TIM1_CH3N/WKUP7/RTC_REFIN"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "STM32F042C6T6_4_1"
			(rectangle
				(start 0 0)
				(end 59.69 -43.18)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type color)
					(color 255 255 194 1)
				)
			)
		)
		(embedded_fonts no)
	)
)
