(footprint "VSS8D3M6-M3_I" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 2.032 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5e4fd939-55f6-47f0-8153-09e6fb69f879)
  )
  (fp_text value "VSS8D3M6-M3_I" (at 0 -2.286 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7b973015-67b6-495a-85ee-d32e2cbf23e6)
  )
  (fp_text user "${REFERENCE}" (at 0 -3.81 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e781cd21-f816-4e74-8072-7871164d9b65)
  )
  (fp_line (start -2.032 -1.27) (end 2.032 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 23c245f6-de70-4261-ba8f-d1eea5084be3))
  (fp_line (start -0.508 -0.762) (end -0.508 0.762) (layer "F.SilkS") (width 0.12) (tstamp 3d443b04-7d1e-44fc-b355-6efe68ddf51e))
  (fp_line (start -2.032 1.27) (end 2.032 1.27) (layer "F.SilkS") (width 0.12) (tstamp b63b1563-2989-4ee9-ac96-1797861a9c27))
  (fp_poly (pts
      (xy 0.508 0.762)
      (xy -0.508 0)
      (xy 0.508 -0.762)
    ) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 59ffeb3d-d92e-4172-ac6a-a2c964cb961d))
  (pad "1" smd rect (at -1.525 0) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d073503e-4e48-46cc-bcbe-caf1902ce00d))
  (pad "2" smd rect (at 1.525 0) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 76f4db9a-acab-4870-936f-51623cef9239))
  (model "${KIPRJMOD}/libraries/DO-221.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
