(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MAX668EUB+T" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 26.67 -12.7 0)
      (effects (font (size 1.524 1.524)) (justify left))
    )
    (property "Value" "MAX668EUB+T" (id 1) (at 26.67 -10.16 0)
      (effects (font (size 1.524 1.524)) (justify left))
    )
    (property "Footprint" "maxim:MAX668EUB&plus_T" (id 2) (at 26.67 -10.16 0)
      (effects (font (size 1.524 1.524)) (justify left) hide)
    )
    (property "Datasheet" "https://www.mouser.be/datasheet/2/256/MAX668-MAX669-1515952.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "ki_fp_filters" "21-0061L_MXM 21-0061L_MXM-M 21-0061L_MXM-L" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX668EUB+T_1_1"
      (polyline
        (pts
          (xy 7.62 -7.62)
          (xy 33.02 -7.62)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 7.62 5.08)
          (xy 7.62 -7.62)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 33.02 -7.62)
          (xy 33.02 5.08)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 33.02 5.08)
          (xy 7.62 5.08)
        )
        (stroke (width 0.127) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin output line (at 5.08 -2.54 0) (length 2.54)
        (name "LDO" (effects (font (size 1.4986 1.4986))))
        (number "1" (effects (font (size 1.4986 1.4986))))
      )
      (pin input line (at 5.08 2.54 0) (length 2.54)
        (name "SYNC/*SHDN" (effects (font (size 1.4986 1.4986))))
        (number "10" (effects (font (size 1.4986 1.4986))))
      )
      (pin input line (at 5.08 0 0) (length 2.54)
        (name "FREQ" (effects (font (size 1.4986 1.4986))))
        (number "2" (effects (font (size 1.4986 1.4986))))
      )
      (pin power_in line (at 25.4 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.4986 1.4986))))
        (number "3" (effects (font (size 1.4986 1.4986))))
      )
      (pin output line (at 5.08 -5.08 0) (length 2.54)
        (name "REF" (effects (font (size 1.4986 1.4986))))
        (number "4" (effects (font (size 1.4986 1.4986))))
      )
      (pin input line (at 35.56 -5.08 180) (length 2.54)
        (name "FB" (effects (font (size 1.4986 1.4986))))
        (number "5" (effects (font (size 1.4986 1.4986))))
      )
      (pin input line (at 35.56 0 180) (length 2.54)
        (name "CS+" (effects (font (size 1.4986 1.4986))))
        (number "6" (effects (font (size 1.4986 1.4986))))
      )
      (pin power_in line (at 35.56 -2.54 180) (length 2.54)
        (name "PGND" (effects (font (size 1.4986 1.4986))))
        (number "7" (effects (font (size 1.4986 1.4986))))
      )
      (pin output line (at 35.56 2.54 180) (length 2.54)
        (name "EXT" (effects (font (size 1.4986 1.4986))))
        (number "8" (effects (font (size 1.4986 1.4986))))
      )
      (pin power_in line (at 25.4 7.62 270) (length 2.54)
        (name "VCC" (effects (font (size 1.4986 1.4986))))
        (number "9" (effects (font (size 1.4986 1.4986))))
      )
    )
  )
)
