(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "nano 33 IoT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 26.67 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "nano 33 IoT" (id 1) (at -12.7 -33.02 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "arduino:NANO 33 IOT" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "https://docs.arduino.cc/hardware/nano-33-iot" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MF" "Arduino" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "DESCRIPTION" "ATSAMD21G18A Arduino Nano 33 IoT SAM D ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (symbol "nano 33 IoT_0_0"
      (rectangle (start -12.7 25.4) (end 12.7 -30.48)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at 17.78 -15.24 180) (length 5.08)
        (name "D13" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -2.54 0) (length 5.08)
        (name "A6" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -5.08 0) (length 5.08)
        (name "A7" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 20.32 180) (length 5.08)
        (name "VUSB" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 22.86 0) (length 5.08)
        (name "~{RESET}" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -27.94 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 22.86 180) (length 5.08)
        (name "VIN" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -12.7 0) (length 5.08)
        (name "TX" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -10.16 0) (length 5.08)
        (name "RX" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 20.32 0) (length 5.08)
        (name "~{RESET}" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -25.4 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 17.78 180) (length 5.08)
        (name "+3V3" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 12.7 180) (length 5.08)
        (name "D2" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 10.16 180) (length 5.08)
        (name "D3/PWM" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 7.62 180) (length 5.08)
        (name "D4" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 5.08 180) (length 5.08)
        (name "D5/PWM" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 2.54 180) (length 5.08)
        (name "D6/PWM" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 0 180) (length 5.08)
        (name "D7" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -2.54 180) (length 5.08)
        (name "D8" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -5.08 180) (length 5.08)
        (name "D9/PWM" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -7.62 180) (length 5.08)
        (name "D10/PWM" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -10.16 180) (length 5.08)
        (name "D11/MOSI" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 17.78 0) (length 5.08)
        (name "AREF" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 17.78 -12.7 180) (length 5.08)
        (name "D12/MISO" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -17.78 0) (length 5.08)
        (name "+3V3" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -20.32 0) (length 5.08)
        (name "TMS" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -22.86 0) (length 5.08)
        (name "TCLK" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -25.4 0) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -27.94 0) (length 5.08)
        (name "/RESET" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 12.7 0) (length 5.08)
        (name "A0/DAC0" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 10.16 0) (length 5.08)
        (name "A1" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 7.62 0) (length 5.08)
        (name "A2" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 5.08 0) (length 5.08)
        (name "A3" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 2.54 0) (length 5.08)
        (name "A4/SDA" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 0 0) (length 5.08)
        (name "A5/SCL" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
