(footprint "W78C32C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "6616332f-d4f9-4e2c-9023-1f8b42becdc1")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "W78C32C"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a84acbdf-378c-4081-93e0-6e2a6e31ea86")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f2391eb-6eb1-40f1-9e1b-fe18a733c0df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "23b81288-4b37-438d-bb6a-0a1d4a18cdef")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -8.3 -8.3)
		(end 8.3 8.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "ba1bfe56-975c-4a1c-91de-4ddde18ced3f")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6b309b0e-9054-4909-ba76-07b5d6a163d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d27f6ada-877f-43f8-9970-912ea89539b2")
	)
	(pad "2" thru_hole circle
		(at -1.27 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1dcf2a4f-59c2-430c-9d88-0a00457aead9")
	)
	(pad "3" thru_hole circle
		(at -2.54 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "59d17bb6-0e8f-4a86-b208-b1fbb36b0d9e")
	)
	(pad "4" thru_hole circle
		(at -3.81 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0f98770b-d9ab-440e-bfb7-9009f7c937a8")
	)
	(pad "5" thru_hole circle
		(at -5.08 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "712d1499-ceea-4ba2-b343-30a8a5718488")
	)
	(pad "6" thru_hole circle
		(at -6.35 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c25024ef-bbac-4000-88d5-3440321864f0")
	)
	(pad "7" thru_hole circle
		(at -8.3 -6.35 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1e9f5ba4-bbc3-427a-964e-a16f1fe1f26e")
	)
	(pad "8" thru_hole circle
		(at -8.3 -5.08 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7090339e-0a16-4724-b202-1d4570d4201f")
	)
	(pad "9" thru_hole circle
		(at -8.3 -3.81 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c4da1b7b-3f84-4c8a-96ef-f830a7e5d552")
	)
	(pad "10" thru_hole circle
		(at -8.3 -2.54 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b364ce73-24dc-42c0-ab07-e5cadeee0820")
	)
	(pad "11" thru_hole circle
		(at -8.3 -1.27 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8c7e59eb-5a97-4e66-b05e-23acfcfa2e6a")
	)
	(pad "12" thru_hole circle
		(at -8.3 0 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2c890d6a-954c-4896-9abe-25c3c57a2637")
	)
	(pad "13" thru_hole circle
		(at -8.3 1.27 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "35055336-7a56-44f2-90a4-bc10a06628ad")
	)
	(pad "14" thru_hole circle
		(at -8.3 2.54 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dde36691-918e-4a8f-9592-6453d63cf4c3")
	)
	(pad "15" thru_hole circle
		(at -8.3 3.81 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a4455b93-54a5-4fab-a4c0-d14faf46141f")
	)
	(pad "16" thru_hole circle
		(at -8.3 5.08 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f20b95c5-e613-424b-b5e1-ced43f305458")
	)
	(pad "17" thru_hole circle
		(at -8.3 6.35 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4cd82151-5acd-4244-b222-e2a3a8a036fd")
	)
	(pad "18" thru_hole circle
		(at -6.35 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "83119c88-31c9-4b33-a219-35c962bdbb53")
	)
	(pad "19" thru_hole circle
		(at -5.08 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dd795b80-0745-41c2-81e3-ef4cab0754a4")
	)
	(pad "20" thru_hole circle
		(at -3.81 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b0b710dd-3eb8-4957-947e-1728a8d7ea27")
	)
	(pad "21" thru_hole circle
		(at -2.54 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "eb3410f9-4b87-4536-b6b0-6fb736518053")
	)
	(pad "22" thru_hole circle
		(at -1.27 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a9bfff20-895e-470c-b5ae-e7bcb618c47a")
	)
	(pad "23" thru_hole circle
		(at 0 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2e5348f0-e2ce-409c-a2b8-7d89b43d022d")
	)
	(pad "24" thru_hole circle
		(at 1.27 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "985975c0-69c4-416f-b67b-0dfb62ae3943")
	)
	(pad "25" thru_hole circle
		(at 2.54 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8f2947fb-65e2-424f-b5d4-879fef993b05")
	)
	(pad "26" thru_hole circle
		(at 3.81 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6b15a8a5-8441-4a84-858f-9ed3f65228c4")
	)
	(pad "27" thru_hole circle
		(at 5.08 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3d9d914e-0ae0-4da9-bd4b-413154be5457")
	)
	(pad "28" thru_hole circle
		(at 6.35 8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5843a987-2f5c-44db-8043-88b683a4eb66")
	)
	(pad "29" thru_hole circle
		(at 8.3 6.35 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e331b4b0-cd05-4a2b-a0b9-77864156d7eb")
	)
	(pad "30" thru_hole circle
		(at 8.3 5.08 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c9a52bd9-8e01-4583-8663-920943c4143e")
	)
	(pad "31" thru_hole circle
		(at 8.3 3.81 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "77ca3f12-3c66-48c6-bd6d-f81ed3926021")
	)
	(pad "32" thru_hole circle
		(at 8.3 2.54 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e27076e0-3a80-4355-a95b-75910077a27a")
	)
	(pad "33" thru_hole circle
		(at 8.3 1.27 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c2d792df-557d-4480-bc9e-31a08b9c83d0")
	)
	(pad "34" thru_hole circle
		(at 8.3 0 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4fd03167-25ae-48fd-b05b-fccecd1e8334")
	)
	(pad "35" thru_hole circle
		(at 8.3 -1.27 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bc244773-0565-4be3-acec-e290362c2d92")
	)
	(pad "36" thru_hole circle
		(at 8.3 -2.54 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "653df5a8-3603-4105-b51f-d0fc3e3a8258")
	)
	(pad "37" thru_hole circle
		(at 8.3 -3.81 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8b1bfdf7-a973-4408-92b6-cfed06e45d32")
	)
	(pad "38" thru_hole circle
		(at 8.3 -5.08 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a545e07d-994f-4957-ac10-a74bdd1cb56b")
	)
	(pad "39" thru_hole circle
		(at 8.3 -6.35 90)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d5edb0af-9e9e-4d62-92b8-aeb10769633e")
	)
	(pad "40" thru_hole circle
		(at 6.35 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a969a06a-57cd-4e54-89ab-8c8b67223bad")
	)
	(pad "41" thru_hole circle
		(at 5.08 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "92ba6519-f03a-4197-b620-1c4eb0b3f600")
	)
	(pad "42" thru_hole circle
		(at 3.81 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0c9852d5-4daa-46c6-9d58-94e5a25623a0")
	)
	(pad "43" thru_hole circle
		(at 2.54 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2a7c5280-8907-4df8-b03c-4e797bda3297")
	)
	(pad "44" thru_hole circle
		(at 1.27 -8.3)
		(size 1 1)
		(drill 0.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "11e3f3f9-8ee5-4e06-a902-dbaf3fff9cdd")
	)
	(embedded_fonts no)
)
