(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ATSAMD21G18A" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "ATSAMD21G18A" (id 1) (at 0 -1.27 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm" (id 2) (at 1.27 19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 1.27 19.05 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ATSAMD21G18A_1_1"
      (rectangle (start -13.97 20.32) (end 3.81 0)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -6.35 22.86 270) (length 2.54)
        (name "VDDIO" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -1.27 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 22.86 270) (length 2.54)
        (name "VDDIO" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 10.16 0) (length 2.54)
        (name "/RESET" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -6.35 -2.54 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 6.35 10.16 180) (length 2.54)
        (name "VDDCORE" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 22.86 270) (length 2.54)
        (name "VDDIN" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -2.54 90) (length 2.54)
        (name "GNDANA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 22.86 270) (length 2.54)
        (name "VDDANA" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ATSAMD21G18A_2_1"
      (rectangle (start 0 76.2) (end 6.35 0)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -2.54 74.93 0) (length 2.54)
        (name "PA00" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 62.23 0) (length 2.54)
        (name "PA05" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 59.69 0) (length 2.54)
        (name "PA06" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 57.15 0) (length 2.54)
        (name "PA07" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 54.61 0) (length 2.54)
        (name "PA08" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 52.07 0) (length 2.54)
        (name "PA09" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 49.53 0) (length 2.54)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 46.99 0) (length 2.54)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 72.39 0) (length 2.54)
        (name "PA01" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 44.45 0) (length 2.54)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 41.91 0) (length 2.54)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 39.37 0) (length 2.54)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 36.83 0) (length 2.54)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 34.29 0) (length 2.54)
        (name "PA16" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 31.75 0) (length 2.54)
        (name "PA17" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 29.21 0) (length 2.54)
        (name "PA18" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 26.67 0) (length 2.54)
        (name "PA19" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 24.13 0) (length 2.54)
        (name "PA20" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 69.85 0) (length 2.54)
        (name "PA02" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 21.59 0) (length 2.54)
        (name "PA21" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 19.05 0) (length 2.54)
        (name "PA22" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 16.51 0) (length 2.54)
        (name "PA23" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 13.97 0) (length 2.54)
        (name "PA24" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 11.43 0) (length 2.54)
        (name "PA25" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 8.89 0) (length 2.54)
        (name "PA27" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 67.31 0) (length 2.54)
        (name "PA03" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 6.35 0) (length 2.54)
        (name "PA28" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 3.81 0) (length 2.54)
        (name "PA30" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 1.27 0) (length 2.54)
        (name "PA31" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 64.77 0) (length 2.54)
        (name "PA04" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ATSAMD21G18A_3_1"
      (rectangle (start 0 20.32) (end 6.35 0)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -2.54 8.89 0) (length 2.54)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 6.35 0) (length 2.54)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 3.81 0) (length 2.54)
        (name "PB22" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 1.27 0) (length 2.54)
        (name "PB23" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 19.05 0) (length 2.54)
        (name "PB02" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 16.51 0) (length 2.54)
        (name "PB03" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 13.97 0) (length 2.54)
        (name "PB08" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 11.43 0) (length 2.54)
        (name "PB09" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
