(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "stepstick" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 19.05 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "stepstick" (id 1) (at -12.7 -22.86 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "reprap:stepstick" (id 2) (at -12.7 -25.4 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "https://reprap.org/wiki/StepStick" (id 3) (at -12.7 -25.4 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (symbol "stepstick_0_0"
      (rectangle (start -12.7 -20.32) (end 12.7 17.78)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin input line (at -17.78 15.24 0) (length 5.08)
        (name "EN" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 12.7 180) (length 5.08)
        (name "VCC" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 17.78 -3.81 180) (length 5.08)
        (name "OA1" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 17.78 -1.27 180) (length 5.08)
        (name "OA2" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 17.78 1.27 180) (length 5.08)
        (name "OB1" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 17.78 3.81 180) (length 5.08)
        (name "OB2" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -15.24 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 15.24 180) (length 5.08)
        (name "VMOT" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 7.62 0) (length 5.08)
        (name "MS0" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 5.08 0) (length 5.08)
        (name "MS1" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 2.54 0) (length 5.08)
        (name "MS2" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -17.78 -6.35 0) (length 5.08)
        (name "/RESET" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -17.78 -8.89 0) (length 5.08)
        (name "/SLEEP" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -15.24 0) (length 5.08)
        (name "STEP" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -17.78 0) (length 5.08)
        (name "DIR" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 17.78 -17.78 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
